**AMRL Testing Schedule**

Monday, January 25, 2016

|  |  |  |  |
| --- | --- | --- | --- |
| **Method** | **Description** | **Tester** | **Approximate Time** |
| T 248 | Splitting / Quartering | sgw | 9:00am – 9:30am |
| T 85 | Coarse Aggregate Specific Gravity | sgw | 9:30am – 9:45am |
| T 27 | Sieve Analysis | sgw | 9:30am – 10:00am |
| T 84 | Fine Aggregate Specific Gravity | sgw | 10:00am – 10:30am |
| T 99/180 | Proctor | ftg | 10:30pm – 11:00pm |
| T 89 | Liquid Limit | mmf | 10:45am – 11:00am |
| T 90 | Plastic Limit | mmf | 11:00am – 11:15am |
| T 304 | Fine Aggregate Angularity | sgw | 11:15am – 11:30am |
|  | LUNCH | all | 11:30am – 1:00pm |
| T 308 | Ignition oven | mmf | 11:15am – 11:30am |
| T 87 | Dry prep of soils | sgw | 1:15pm – 1:30pm |
| T 30/11 | Washing | sgw | 1:30pm – 2:00pm |
| R 47 | Reducing HMA sample | mmf | 2:00pm – 2:30pm |
| T 310 | Nuclear Density | mmf | 2:30pm – 3:00pm |
|  | Check equipment / finish up or bulk & rice? | AMRL | 3:00pm – 4:30pm |

Tuesday, January 26, 2016

|  |  |  |  |
| --- | --- | --- | --- |
| **Method** | **Description** | **Tester** | **Approximate Time** |
| Soils/agg | Get dry wts, finish calcs for previous tests | mmf/sgw/ftg | 8:30am – 10:00am |
| T 30 | Washing ignition oven sample? | sgw | 8:45am – 9:15am |
| T 312 | Mix asphalt sample | mmf | 9:15am – 9:30am |
| T 312 | Age the asphalt sample | mmf | 9:30am – 11:30am |
| T 312 | Compact asphalt sample | mmf | 11:30am – 11:45am |
|  | LUNCH | all | 11:45am – 1:15pm |
| T 166 | HMA Bulk sp. gr. (ssd method) | mmf | 1:30pm – 1:45pm |
| T 209 | Gmm (rice method) | mmf | 1:45pm – 2:30pm |
| T 331 | CoreLok | sgw | 2:30pm – 2:45pm |
| T 269 | Calculate air content | sgw | 2:45pm – 3:00pm |
| T 287 | Nuclear AC Content | mmf | 3:00pm – 4:00pm |
| T 329 | Moisture content of HMA | mmf | 4:00pm – 4:15pm |
| R 18 | Review Quality Manual | AMRL | 4:15pm – 5:00pm |